## C89 code generation

The CIF code generator can generate C89 code from a CIF specification. It is assumed the reader of this page is familiar with the general information of the CIF code generator tool. This page describes specific information applicable only to C89 code generation.

In general, use of the C99 code generator is preferred, as the language contains a decade longer development. However, in the case there is no `c99` compiler available, the `c89` code generation might be a useful fallback option to convert a CIF program for controlling a real time system. The conversion uses a simple integrator intended for updating running clocks (derivative should not change during a time step for best results). Also, it does not compute length of the next time step, but instead assumes being called regularly to update internal state and perform discrete steps if possible.

### Supported specifications

The CIF code generator supports a subset of CIF specifications. Generation of C89 code does not impose additional restrictions. See the Supported specifications section of the CIF code generator page for more information.

### Differences in output

When converting a real number to text, for example when printing a real value, the generated C89 code does not preserve trailing zeroes of real number fractions while using `%g`. For example `fmt("%.3g", 1.0)` will output `1` rather than `1.000`.

This may cause real number values to be printed with less digits precision than indicated in the CIF program.

Strings have an upper limit in length that is set during compilation. Longer strings are silently truncated to this length.

### Options

The C89 code generator only uses the common options that apply to all target languages/platforms of the CIF code generator, it has no options of its own.

The code prefix that can be configured using a common option is used to prefix external names, making them unique for the generated code.

### Generated files

C89 code generation leads to creation of seven files:

Generated file | Purpose
--- | ---
`<prefix>_library.h` | Runtime support code and library headers
`<prefix>_library.c` | Runtime support code and library implementation
`<prefix>_engine.h` | Interface definition of the translated CIF program
`<prefix>_engine.c` | Implementation of the translated CIF program
`<prefix>_compile.sh` | Compile script for Linux
`<prefix>_test_code.c` | Example of external functions, allow compiling the generated code
`<prefix>_readme.txt` | Short description of use, the interface, and compile options

where `<prefix>` is replaced by the value of the Code prefix option during code generation.

The aim is to provide a complete and compilable package, to minimize the effort in converting a CIF specification. Most files are static text (modulo the `<prefix>` replacement). The two exceptions are both engine files that contain the C89 version of the CIF specification. The interface of these files is however fixed (modulo the `<prefix>` replacement), and generated data types and operations on them have predictable names, reducing the chance of failed compilation when re-generating the files.

When modifying a generated file (such as the compile script or the example test code), keep in mind that running the code generator again will overwrite all files. Rename a file before modifying it to avoid loss of work.

### Compilation of the generated code

The generated code is C89 code that can be compiled using a C89 C compiler, like `gcc`:

    gcc -Wall -std=c89 -DPRINT_OUTPUT=1 -DCHECK_RANGES=1 \
        <prefix>_engine.c <prefix>_library.c <prefix>_test_code.c -lm

The single `\` is not part of the command, it means the next line should be appended at the end.

The `<prefix>` should be replaced by the value of the Code prefix option during code generation. The `PRINT_OUTPUT` and `CHECK_RANGES` macros enable support for the CIF `print` statement and checking of integer range overlap, as defined by CIF. In general however, you may want to replace the test code file by your own code.

### C89 compile-time options

Besides the `PRINT_OUTPUT` and `CHECK_RANGES` macros, the generated code has a few other compile-time options to customize its behavior. Below is the complete list.

Macro name | Effect
--- | ---
`MAX_STRING_SIZE` | CIF has variable length strings, in the generated code they are converted to strings with a fixed upper limit. Default is 128 (including the terminator character). Set this macro for a different limit. Note that both the library and the engine use this macro. It is crucial that both files use the same value for this macro.
`CHECK_RANGES` | When copying integers from one range to another, where the latter is only partially covered by the former, CIF checks whether the copied values do not violate the destination range. Since violating this property generally indicates a programming error, it is recommended to enable this macro.
`EVENT_OUTPUT` | If set, the generated code calls `<prefix>_InfoEvent()` before and after performing an event to allow third-party code to act on it. Enable if your code needs to know when an event is performed.
`PRINT_OUTPUT` | If set, the CIF `print` statement is performed, and the `<prefix>__PrintOutput()` is called with the resulting text and destination filename. Mainly intended for debugging, but only useful in systems where the text can be displayed to a user.
`MAX_NUM_EVENTS` | The CIF semantics state that execution of edges is instantaneous and time-less. The generated code loops to perform edges, until no edge can be executed any more. Unfortunately, such a loop is not time-less. To avoid requiring too much time, there is an upper limit of 1000 iterations. Set this macro to change the limit.
`KEEP_RUNNING` | The CIF language checks range conversions (if `CHECK_RANGES` is set) and verifies updates of continuous variable updates. Setting this flag disables a few checks. Most of these checks are in `assert()` checks and not controlled by this macro, since violating the condition generally means a crash is eventually inevitable. It is recommended to avoid using this macro.

### Executing the code

The engine files act as a library that implements the CIF program. To run the program, the code must be called regularly. The code has two entry points, one for initializing and performing the first steps, and one for handling a time delay.

The first entry point is:

    <prefix>_EngineFirstStep(void)

This entry point initializes all the data, queries the values of the input variables if present, and performs execution of edges until blocked on the first time step or until hitting the `MAX_NUM_EVENTS` limit. Since this resets the entire CIF program to its initial state, you should only call this when the system being controlled is also (re-)initialized.

The second entry point is more regularly called, after a period of time has passed:

    <prefix>_EngineTimeStep(double delta)

By calling this entry point, you indicate that `delta` (> 0) time units have passed. The code reads new values of the input variables, updates the continuous variables, and performs edges until all edges are blocked, or hitting the `MAX_NUM_EVENTS` limit.

When the call of either entry point returns, you can query the value of the variables to use as input for other parts of the system.

### Environment interface

Calling one of the above entry points causes the CIF program to be executed, up to the next time step (assuming the `MAX_NUM_EVENTS` limit is high enough). During the execution, the code performs a number of callbacks to get information from the environment, to provide information about its actions, or to deliver output. In addition, after each call, variables may be inspected by the environment to get information about the decisions of the CIF program.

The externally provided callback functions that are being used are:

    <prefix>_AssignInputVariables(void)

The CIF program requests new values for all its input variables. In your implementation of this function you should write values directly in the input variables. Input variables are assumed to be independent of other parts of the CIF program, in general you should not need other CIF program values to implement this function.

If `EVENT_OUTPUT` is set during compilation, executed events are reported with:

    <prefix>_InfoEvent(<prefix>_Event_ event, BoolType pre)

If the `EVENT_OUTPUT` macro is set during compilation, the generated code reports with this call that event is about to (`pre` is `TRUE`), or has been (`pre` is `FALSE`) executed. In the pre-event call, the event can be executed, and all variables have their value before performing the updates of the involved edges. In the post-event call, all variables have their values updated as indicated in the updates of the edges.

Primary use of this call is to forward the decision to other parts of the controlled system.

Finally, if the `PRINT_OUTPUT` macro is set during compilation, the generated code reports lines of output to be printed with the following function call:

    <prefix>_PrintOutput(const char *line, const char *fname)

It denotes that text `line` should be printed at file `fname`. The primary uses of this call are to enable debugging the system, or to log relevant events. Note that `fname` here can mean anything. It can mean a real file, but also a pseudo-device like `:stdout` which is commonly used to print output to the C `stdout` stream.

### Data access

Each CIF constant is available as a variable that does not change after initialization. Each algebraic variable can be queried by calling a function with the same name as the variable. The value of continuous variables is available by accessing the equivalent variable in the generated code. The derivative of each continuous variable is available as function named by the variable, and the suffix `deriv`. The model time is available as `model_time`. There is no derivative function of time. Internal functions are available as well if required.

The engine header file lists the translated names. It should be easy to find the relevant entry, as the generated code also documents the original name.

### Data types

The following table defines how CIF data types are converted in the C89 generated code.

CIF data type | C89 data type
--- | ---
`bool` | `BoolType` which is a typedef to `int`
`int` | `IntType` which is a typedef to `int`
`enum e = ...` | `<prefix>Enum` which is a typedef to `enum Enum<prefix>_`
`real` | `RealType` which is a typedef to `double`
`string` | `StringType` which is a typedef to a `struct`
`list[n] t` | `...Type` which is a typedef to a `struct`
`tuple(...)` | `...Type` which is a typedef to a `struct`

A few notes:

- The `...` in the C89 `...Type` name for arrays (fixed length lists) and tuples is the systematic type name of the array or tuple type.

- Due to preprocessing all enumerations are merged into one. The generated C89 code always has exactly one translated `enum`.

- The elementary data types (`BoolType`, `IntType`, `RealType`, and `StringType`) are defined in the library header file.

- The `StringType` structure wraps a `char data[MAX_STRING_SIZE]` array. The `struct` allows copying arrays by value using an assignment statement.

- The array type (list with a fixed length) structure wraps a `<element-type> data[<size>]` array for the same reason. Copying an array by assignment is allowed.

- The tuple type is a structure with fields `_field0`, `_field1`, and so on, where the type of each field in the structure matches with the type of the CIF tuple field.

- Boolean constants `true` and `false` are named `TRUE` and `FALSE` respectively.

- The `-0.0` value of doubles gets replaced by `0.0` to void subtle equality problems.

- Strings get silently truncated to `MAX_STRING_SIZE - 1` characters. They are always terminated with a NUL character.

- Enumeration values get `_<prefix>_` added in front to make them unique.

### Systematic type names

For tuple and list types, the type is converted to a name in a systematic way, making each type unique and predictable.

The conversion composes a name of a type from the type of its elements, and concatenates the result. The following conversion table applies:

CIF type | Systematic name
--- | ---
`bool` | `B`
`int` | `I`
`enum e = ...` | `E` (Due to linearization, all enumerations are merged together to a single enumeration. As such, always exactly one `enum` is generated for a CIF model.)
`real` | `R`
`list[n] t` | `A<n><t>`, with `<n>` the length of the array, and `<t>` the systematic type name of the element type of the array.
`tuple(t1, t2, t3, ..., tn)` | `T<n><t1><t2><t3>...<tn>`, with `<n>` the number of fields in the tuple, and `<t1>` to `<tn>` the systematic type names of the fields.

For example, type `list[5] int` is converted to `A5I`, and type `tuple(list[5] int x; tuple(real a, b) z)` is converted to `T2A5IT2RR` (concatenation of `T2` with the field type names `A5I` and `T2RR`).

### Runtime errors

The CIF language defines strict sets of allowed values for all data types, and performs checking of these values at run time. The generated C89 code follows that idea, and checks whether operations on data are safe. Most of these checks are performed with an `assert`. Executed C code does not provide useful stack traces by default, and original line numbers of e.g. a CIF program have no meaning due to the linearization that is performed before code is generated. In addition, the generated code is quite readable and it is not too hard to understand what the code is doing at some C source line.